wan과 lan의 ni가 동일 : 브릿지 모드
wan과 lan의 ni가 상이 : 라우터 모드

zfs : zettabyte file system - 안정성이 높다
ufs : unix file system - 휘발성 메모리

utm 장비



pfsense 설치, IPS 환경 구축
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Status / Dashboard

System Information

Name
User

system

BIOS

Version

CPU Type

Hardware crypto

Kernel PTI

pfSense home arpa
admin@192.168.0.20 (Local Database)

VMware Virtual Machine

Netgate Device ID: 25705f50d036772440c0

Vendor: Phoenix Technologies LTD
Version: 6.00

Release Date: Mon Mar 24 2025
Boot Method: BIOS.

2.8.1-RELEASE (amd64)
built on Wed Jul 1 6:25:00 09 2026
FreeBSD 15.0-CURRENT

Error in version information &'

AMD Ryzen 5 3600 6-Core Processor
2CPUs - 1 package(s) x 2 core(s)
AES-NI CPU Crypto: Yes (inactive)
QAT Crypto: No

Inactive
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Netgate Services And Support 00

Contract Type  Community Support
Community Support Only

NETGATE & PFSENSE COMMUNITY SUPPORT RESOURCES

If you purchased your pfSense gateway firewall appliance from
Netgate and elected Community Support at the point of sale o
installed pfSense on your own hardware, you have access to
various community support resources. This includes the NETGATE
RESOURCE LIBRARY.

You also may upgrade to a Netgate Global Technical Assistance
Center (TAC) Support subscription. We're always ont Our team is
staffed 24x7x365 and committed to elivering enterprise-ciass,
worldwide support at a price point that i more than competitive
when compared to others in our space.

- Community Support

- Upgrade Your Support Resources

+ Nelgate Global Support - Official pfSense Training by
FAQ Netgate

. i v
Netgate Professional e et o




